

Reading the command file, zdrive.inp.phg.ipm.fixed03
Input values:
  Zoltan version 3.601
  zdrive version 1.0
  Total number of Processors = 4

  Performing load balance using hypergraph.
	Parameters:
		lb_approach partition
		hypergraph_package phg
		phg_coarsening_method ipm
		phg_output_level 1
		phg_coarsening_limit 1
		num_global_parts 7
		phg_coarsepartition_method linear
		remap 0

  Initially distribute input objects in linear fashion (first n/p to process 0, etc).

  Distribute pins so each process gets full rows.
##########################################################
ZOLTAN Load balancing method = 11 (HYPERGRAPH)
Starting iteration 1

BEFORE load balancing
DRIVER EVAL:  load:  max 7.000000  min 6.000000  sum 25.000000
DRIVER EVAL:  objs:  max 7  min 6  sum 25
DRIVER EVAL:  cuts:  max 12  min 6  sum 36

Zoltan_LB_Eval_Balance  Part count: 7 requested, 4 actual , 4 non-empty
Zoltan_LB_Eval_Balance  Statistics with respect to 4 parts: 
Zoltan_LB_Eval_Balance                             Min      Max      Sum  Imbalance
Zoltan_LB_Eval_Balance  Number of objects  :         6        7       25     1.960



Zoltan_LB_Eval_Graph  Part count: 7 requested, 4 actual, 4 non-empty
Zoltan_LB_Eval_Graph  Statistics with respect to 4 parts: 
Zoltan_LB_Eval_Graph                             Min      Max      Sum  Imbalance
Zoltan_LB_Eval_Graph  Number of objects  :         6        7       25     1.96

Zoltan_LB_Eval_Graph  Statistics with respect to 4 parts: 
Zoltan_LB_Eval_Graph                                    Min      Max    Average    Sum
Zoltan_LB_Eval_Graph  Num boundary objects      :         5        6      5.5       22
Zoltan_LB_Eval_Graph  Number of cut edges       :         6       12        9       36
Zoltan_LB_Eval_Graph  Num Nbor Parts            :         1        2      1.5        6



Zoltan_LB_Eval_HG  Part count: 7 requested, 4 actual, 4 non-empty
Zoltan_LB_Eval_HG  Statistics with respect to 4 parts: 
Zoltan_LB_Eval_HG                            Min      Max     Sum  Imbalance
Zoltan_LB_Eval_HG  Number of objects :         6        7       25   1.960
Zoltan_LB_Eval_HG  Object weight     :         6        7       25   1.960

Zoltan_LB_Eval_HG  CUTN (Sum_edges( (#parts(edge)>1)*ewgt )):   22.000
Zoltan_LB_Eval_HG  CUTL (Sum_edges( (#parts(edge)-1)*ewgt )):   30.000
Zoltan_LB_Eval_HG  CUTL-MAX (Max_parts( comm. volume ):         10.000


Build configuration:

  ZOLTAN_ID_TYPE: unsigned long (8 bytes)
  ZOLTAN_GNO_TYPE: ssize_t, (8 bytes)
  MPI_Datatype for ZOLTAN_ID_TYPE: MPI_UNSIGNED_LONG
  MPI_Datatype for ZOLTAN_GNO_TYPE: MPI_LONG
  Third party library: ParMetis version 3.1
  Third party library: PTScotch   Third party library: Scotch 
ZOLTAN Parameter IMBALANCE_TOL[0] = 1.100000
ZOLTAN Parameter AUTO_MIGRATE = FALSE
ZOLTAN Parameter MIGRATE_ONLY_PROC_CHANGES = 1
ZOLTAN Parameter OBJ_WEIGHT_DIM = 0
ZOLTAN Parameter EDGE_WEIGHT_DIM = 0
ZOLTAN Parameter DEBUG_LEVEL = 1
ZOLTAN Parameter DEBUG_PROCESSOR = 0
ZOLTAN Parameter DETERMINISTIC = TRUE
ZOLTAN Parameter TIMER = 1 (wall)
ZOLTAN Parameter NUM_GID_ENTRIES = 1
ZOLTAN Parameter NUM_LID_ENTRIES = 1
ZOLTAN Parameter RETURN_LISTS = IMPORT AND EXPORT
ZOLTAN Parameter NUM_GLOBAL_PARTS = 7
ZOLTAN Parameter NUM_LOCAL_PARTS = -1
ZOLTAN Parameter REMAP = 0
ZOLTAN Parameter SEED = 1220988223 (1220988223)
ZOLTAN Parameter LB_APPROACH = PARTITION
ZOLTAN Parameter HYPERGRAPH_PACKAGE = PHG
ZOLTAN Parameter PHG_MULTILEVEL = 1
ZOLTAN Parameter PHG_CUT_OBJECTIVE = connectivity
ZOLTAN Parameter PHG_OUTPUT_LEVEL = 1
ZOLTAN Parameter FINAL_OUTPUT = 0
ZOLTAN Parameter CHECK_GRAPH = 0
ZOLTAN Parameter CHECK_HYPERGRAPH = 0
ZOLTAN Parameter PHG_NPROC_VERTEX = -1
ZOLTAN Parameter PHG_NPROC_EDGE = -1
ZOLTAN Parameter PHG_COARSENING_LIMIT = 1
ZOLTAN Parameter PHG_COARSENING_NCANDIDATE = 100
ZOLTAN Parameter PHG_COARSENING_METHOD = IPM
ZOLTAN Parameter PHG_COARSENING_METHOD_FAST = l-ipm
ZOLTAN Parameter PHG_VERTEX_VISIT_ORDER = 0
ZOLTAN Parameter PHG_EDGE_SCALING = 0
ZOLTAN Parameter PHG_VERTEX_SCALING = 0
ZOLTAN Parameter PHG_COARSEPARTITION_METHOD = LINEAR
ZOLTAN Parameter PHG_REFINEMENT_METHOD = fm2
ZOLTAN Parameter PHG_DIRECT_KWAY = 0
ZOLTAN Parameter PHG_REFINEMENT_LOOP_LIMIT = 10
ZOLTAN Parameter PHG_REFINEMENT_MAX_NEG_MOVE = 250
ZOLTAN Parameter PHG_REFINEMENT_QUALITY = 1.000000
ZOLTAN Parameter PHG_USE_TIMERS = 0
ZOLTAN Parameter USE_TIMERS = 0
ZOLTAN Parameter PHG_EDGE_SIZE_THRESHOLD = 0.250000
ZOLTAN Parameter PHG_MATCH_EDGE_SIZE_THRESHOLD = 500
ZOLTAN Parameter PHG_BAL_TOL_ADJUSTMENT = 0.700000
ZOLTAN Parameter PHG_EDGE_WEIGHT_OPERATION = max
ZOLTAN Parameter PARKWAY_SERPART = patoh
ZOLTAN Parameter ADD_OBJ_WEIGHT = none
ZOLTAN Parameter PHG_RANDOMIZE_INPUT = 0
ZOLTAN Parameter PHG_PROCESSOR_REDUCTION_LIMIT = 0.000000
ZOLTAN Parameter PHG_REPART_MULTIPLIER = 100.000000
ZOLTAN Parameter HYBRID_REDUCTION_FACTOR = 0.100000
ZOLTAN Parameter HYBRID_REDUCTION_LEVELS = 2147483647
ZOLTAN Parameter PATOH_ALLOC_POOL0 = 0
ZOLTAN Parameter PATOH_ALLOC_POOL1 = 0
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   0 |V|=    12 |E|=    12 #pins=    27 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   0 |V|=    12 |E|=    13 #pins=    23 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   0 |V|=    13 |E|=    13 #pins=    31 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   0 |V|=    13 |E|=    12 #pins=    24 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   1 |V|=     6 |E|=    14 #pins=    19 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   1 |V|=     6 |E|=    11 #pins=    16 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   1 |V|=     8 |E|=    14 #pins=    29 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   1 |V|=     8 |E|=    11 #pins=    20 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   2 |V|=     5 |E|=     4 #pins=    10 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   2 |V|=     3 |E|=     4 #pins=     3 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   2 |V|=     5 |E|=    12 #pins=    19 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   2 |V|=     3 |E|=    12 #pins=    12 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   3 |V|=     2 |E|=     3 #pins=     4 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   3 |V|=     2 |E|=     3 #pins=     4 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   3 |V|=     2 |E|=     2 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   3 |V|=     2 |E|=     2 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   4 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   4 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 2, 2] ->START   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->START   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->START   5 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 1, 1)/[ 2, 2] ->START   5 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 1, 0)/[ 2, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   5 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   5 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   4 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   4 |V|=     1 |E|=     1 #pins=     1 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   3 |V|=     2 |E|=     3 #pins=     4 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   3 |V|=     2 |E|=     3 #pins=     4 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   3 |V|=     2 |E|=     2 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   3 |V|=     2 |E|=     2 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.75 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   2 |V|=     3 |E|=     4 #pins=     3 1/IPM/LINEAR/fm2 p=2 bal=1.19 cutl=15.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   2 |V|=     5 |E|=     4 #pins=    10 1/IPM/LINEAR/fm2 p=2 bal=1.19 cutl=15.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   2 |V|=     3 |E|=    12 #pins=    12 1/IPM/LINEAR/fm2 p=2 bal=1.19 cutl=15.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   2 |V|=     5 |E|=    12 #pins=    19 1/IPM/LINEAR/fm2 p=2 bal=1.19 cutl=15.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   1 |V|=     6 |E|=    14 #pins=    19 1/IPM/LINEAR/fm2 p=2 bal=1.05 cutl=15.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   1 |V|=     8 |E|=    14 #pins=    29 1/IPM/LINEAR/fm2 p=2 bal=1.05 cutl=15.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   1 |V|=     6 |E|=    11 #pins=    16 1/IPM/LINEAR/fm2 p=2 bal=1.05 cutl=15.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   1 |V|=     8 |E|=    11 #pins=    20 1/IPM/LINEAR/fm2 p=2 bal=1.05 cutl=15.00
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   0 |V|=    12 |E|=    12 #pins=    27 1/IPM/LINEAR/fm2 p=2 bal=1.03 cutl=14.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   0 |V|=    13 |E|=    12 #pins=    24 1/IPM/LINEAR/fm2 p=2 bal=1.03 cutl=14.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   0 |V|=    12 |E|=    13 #pins=    23 1/IPM/LINEAR/fm2 p=2 bal=1.03 cutl=14.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   0 |V|=    13 |E|=    13 #pins=    31 1/IPM/LINEAR/fm2 p=2 bal=1.03 cutl=14.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->Rdivide(0, 6): 14.0
| 2/ 4|: ( 0, 1)/[ 2, 2] ->Rdivide(0, 6): 14.0
| 0/ 4|: ( 0, 0)/[ 2, 2] ->Rdivide(0, 6): 14.0
| 3/ 4|: ( 1, 1)/[ 2, 2] ->Rdivide(0, 6): 14.0
| 2/ 4|: ( 0, 1)/[ 2, 2] ->Left: H(2, 8, 0) ----> H(0, 0, 0) Weights=(14.00, 11.00)
| 3/ 4|: ( 1, 1)/[ 2, 2] ->Left: H(12, 8, 26) ----> H(0, 0, 0) Weights=(14.00, 11.00)
| 0/ 4|: ( 0, 0)/[ 2, 2] ->Left: H(2, 9, 6) ----> H(14, 9, 31) Weights=(14.00, 11.00)
| 1/ 4|: ( 1, 0)/[ 2, 2] ->Left: H(12, 9, 23) ----> H(14, 8, 24) Weights=(14.00, 11.00)
| 1/ 4|: ( 1, 0)/[ 2, 2] ->Right: H(1, 8, 1) ----> H(0, 0, 0) Weights=(14.00, 11.00)
| 1/ 4|: ( 1, 0)/[ 2, 2] ->Left: H(14, 8, 24) OldI: 1.10 NewI: 1.12
| 0/ 4|: ( 0, 0)/[ 2, 2] ->Right: H(10, 8, 19) ----> H(0, 0, 0) Weights=(14.00, 11.00)
| 0/ 4|: ( 0, 0)/[ 2, 2] ->Left: H(14, 9, 31) OldI: 1.10 NewI: 1.12
| 2/ 4|: ( 0, 1)/[ 2, 2] ->Right: H(10, 7, 21) ----> H(11, 8, 23) Weights=(14.00, 11.00)
| 3/ 4|: ( 1, 1)/[ 2, 2] ->Right: H(1, 7, 2) ----> H(11, 7, 20) Weights=(14.00, 11.00)
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   0 |V|=    14 |E|=     9 #pins=    31 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 1)/[ 2, 2] ->Right: H(11, 8, 23) OldI: 1.10 NewI: 1.07
| 3/ 4|: ( 1, 1)/[ 2, 2] ->Right: H(11, 7, 20) OldI: 1.10 NewI: 1.07
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   0 |V|=    14 |E|=     8 #pins=    24 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   0 |V|=    11 |E|=     8 #pins=    23 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   0 |V|=    11 |E|=     7 #pins=    20 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   1 |V|=     6 |E|=     2 #pins=     4 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   1 |V|=     6 |E|=     6 #pins=    16 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   1 |V|=     8 |E|=     6 #pins=    19 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   1 |V|=     8 |E|=     7 #pins=    19 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   2 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   2 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   2 |V|=     5 |E|=     2 #pins=     7 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   2 |V|=     5 |E|=     6 #pins=    14 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   3 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   3 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   3 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   3 |V|=     3 |E|=     3 #pins=     7 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   4 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   4 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   3 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   3 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   2 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   2 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   1 |V|=     6 |E|=     2 #pins=     4 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   1 |V|=     6 |E|=     6 #pins=    16 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   0 |V|=    11 |E|=     8 #pins=    23 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   0 |V|=    11 |E|=     7 #pins=    20 1/IPM/LINEAR/fm2 p=2 bal=1.09 cutl=4.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->Rdivide(4, 6): 4.0
| 3/ 4|: ( 0, 1)/[ 1, 2] ->Rdivide(4, 6): 4.0
| 2/ 4|: ( 0, 0)/[ 1, 2] ->Left: H(8, 7, 20) OldI: 1.07 NewI: 0.98
| 3/ 4|: ( 0, 1)/[ 1, 2] ->Left: H(8, 6, 12) OldI: 1.07 NewI: 0.98
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   0 |V|=     8 |E|=     7 #pins=    20 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   0 |V|=     8 |E|=     6 #pins=    12 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->START   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->START   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   5 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   4 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=1.86 cutl=4.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   4 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.86 cutl=4.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   3 |V|=     3 |E|=     3 #pins=     7 1/IPM/LINEAR/fm2 p=2 bal=1.86 cutl=4.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   3 |V|=     3 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.86 cutl=4.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   2 |V|=     5 |E|=     2 #pins=     7 1/IPM/LINEAR/fm2 p=2 bal=1.43 cutl=9.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   2 |V|=     5 |E|=     6 #pins=    14 1/IPM/LINEAR/fm2 p=2 bal=1.43 cutl=9.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   1 |V|=     8 |E|=     6 #pins=    19 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=11.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   1 |V|=     8 |E|=     7 #pins=    19 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=11.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   1 |V|=     4 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   1 |V|=     4 |E|=     4 #pins=     9 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   0 |V|=    14 |E|=     9 #pins=    31 1/IPM/LINEAR/fm2 p=2 bal=1.00 cutl=9.00
| 1/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   0 |V|=    14 |E|=     8 #pins=    24 1/IPM/LINEAR/fm2 p=2 bal=1.00 cutl=9.00
| 0/ 4|: ( 0, 0)/[ 1, 2] ->Rdivide(0, 3): 9.0
| 1/ 4|: ( 0, 1)/[ 1, 2] ->Rdivide(0, 3): 9.0
| 0/ 4|: ( 0, 0)/[ 1, 2] ->Left: H(7, 7, 17) ----> H(7, 10, 23) Weights=(7.00, 7.00)
| 1/ 4|: ( 0, 1)/[ 1, 2] ->Left: H(7, 3, 6) ----> H(0, 0, 0) Weights=(7.00, 7.00)
| 0/ 4|: ( 0, 0)/[ 1, 2] ->Right: H(7, 4, 11) ----> H(0, 0, 0) Weights=(7.00, 7.00)
| 0/ 4|: ( 0, 0)/[ 1, 2] ->Left: H(7, 10, 23) OldI: 1.12 NewI: 1.12
| 1/ 4|: ( 0, 1)/[ 1, 2] ->Right: H(7, 5, 14) ----> H(7, 9, 25) Weights=(7.00, 7.00)
| 0/ 4|: ( 0, 0)/[ 1, 1] ->START   0 |V|=     7 |E|=    10 #pins=    23 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 1)/[ 1, 2] ->Right: H(7, 9, 25) OldI: 1.12 NewI: 1.12
| 1/ 4|: ( 0, 0)/[ 1, 1] ->START   0 |V|=     7 |E|=     9 #pins=    25 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   2 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   2 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 1] ->START   1 |V|=     4 |E|=     3 #pins=     6 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 0)/[ 1, 1] ->START   1 |V|=     4 |E|=     6 #pins=    14 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 1] ->START   2 |V|=     3 |E|=     2 #pins=     4 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 0)/[ 1, 1] ->START   2 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 0/ 4|: ( 0, 0)/[ 1, 1] ->START   3 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 0)/[ 1, 1] ->START   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 0)/[ 1, 1] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 1/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 1/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   2 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=4.00
| 1/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   1 |V|=     4 |E|=     6 #pins=    14 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=4.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->START   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 1/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   0 |V|=     7 |E|=     9 #pins=    25 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=4.00
| 1/ 4|: ( 0, 0)/[ 1, 1] ->Rdivide(2, 3): 4.0
| 0/ 4|: ( 0, 0)/[ 1, 1] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   4 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   3 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   2 |V|=     3 |E|=     2 #pins=     4 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   1 |V|=     4 |E|=     3 #pins=     6 1/IPM/LINEAR/fm2 p=2 bal=1.43 cutl=3.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->FINAL   0 |V|=     7 |E|=    10 #pins=    23 1/IPM/LINEAR/fm2 p=2 bal=1.14 cutl=2.00
| 0/ 4|: ( 0, 0)/[ 1, 1] ->Rdivide(0, 1): 2.0
| 2/ 4|: ( 0, 0)/[ 1, 2] ->START   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 3/ 4|: ( 0, 1)/[ 1, 2] ->START   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2...
| 2/ 4|: ( 0, 0)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->Local Ratio Cut= 0.00   Global Ratio Cut= 0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   3 |V|=     1 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   2 |V|=     2 |E|=     0 #pins=     0 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   2 |V|=     2 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=2.00 cutl=0.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   1 |V|=     4 |E|=     1 #pins=     2 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=4.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   1 |V|=     4 |E|=     4 #pins=     9 1/IPM/LINEAR/fm2 p=2 bal=1.50 cutl=4.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->FINAL   0 |V|=     8 |E|=     7 #pins=    20 1/IPM/LINEAR/fm2 p=2 bal=1.25 cutl=4.00
| 3/ 4|: ( 0, 1)/[ 1, 2] ->FINAL   0 |V|=     8 |E|=     6 #pins=    12 1/IPM/LINEAR/fm2 p=2 bal=1.25 cutl=4.00
| 2/ 4|: ( 0, 0)/[ 1, 2] ->Rdivide(4, 5): 4.0
| 3/ 4|: ( 0, 1)/[ 1, 2] ->Rdivide(4, 5): 4.0
| 0/ 4|: ( 0, 0)/[ 2, 2] ->FINAL   0 |V|=    12 |E|=    12 #pins=    27 IPM/LINEAR/fm2 p=7 bal=1.40 cutl=37.00
| 1/ 4|: ( 1, 0)/[ 2, 2] ->FINAL   0 |V|=    13 |E|=    12 #pins=    24 IPM/LINEAR/fm2 p=7 bal=1.40 cutl=37.00
| 2/ 4|: ( 0, 1)/[ 2, 2] ->FINAL   0 |V|=    12 |E|=    13 #pins=    23 IPM/LINEAR/fm2 p=7 bal=1.40 cutl=37.00
| 3/ 4|: ( 1, 1)/[ 2, 2] ->FINAL   0 |V|=    13 |E|=    13 #pins=    31 IPM/LINEAR/fm2 p=7 bal=1.40 cutl=37.00
Proc 1: Calls to malloc = 3969,  Calls to free = 3969
Proc 2: Calls to malloc = 3546,  Calls to free = 3546
Proc 3: Calls to malloc = 3643,  Calls to free = 3643
Proc 0: Calls to malloc = 4049,  Calls to free = 4049

DRIVER:  Zoltan_LB_Partition time = 0.101813
DRIVER:  new_decomp 1 Min/Max Import: 3 9
DRIVER:  new_decomp 1 Min/Max Export: 5 7
DRIVER:  Total migration time = 0.00223804
0:  All fixed objects are correct.

AFTER load balancing
DRIVER EVAL:  load:  max 9.000000  min 4.000000  sum 25.000000
DRIVER EVAL:  objs:  max 9  min 4  sum 25
DRIVER EVAL:  cuts:  max 16  min 7  sum 48

Zoltan_LB_Eval_Balance  Part count: 7 requested, 7 actual , 7 non-empty
Zoltan_LB_Eval_Balance  Statistics with respect to 7 parts: 
Zoltan_LB_Eval_Balance                             Min      Max      Sum  Imbalance
Zoltan_LB_Eval_Balance  Number of objects  :         3        5       25     1.400



Zoltan_LB_Eval_Graph  Part count: 7 requested, 7 actual, 7 non-empty
Zoltan_LB_Eval_Graph  Statistics with respect to 7 parts: 
Zoltan_LB_Eval_Graph                             Min      Max      Sum  Imbalance
Zoltan_LB_Eval_Graph  Number of objects  :         3        5       25      1.4

Zoltan_LB_Eval_Graph  Statistics with respect to 7 parts: 
Zoltan_LB_Eval_Graph                                    Min      Max    Average    Sum
Zoltan_LB_Eval_Graph  Num boundary objects      :         3        4     3.43       24
Zoltan_LB_Eval_Graph  Number of cut edges       :         5       14     7.43       52
Zoltan_LB_Eval_Graph  Num Nbor Parts            :         2        4     2.86       20



Zoltan_LB_Eval_HG  Part count: 7 requested, 7 actual, 7 non-empty
Zoltan_LB_Eval_HG  Statistics with respect to 7 parts: 
Zoltan_LB_Eval_HG                            Min      Max     Sum  Imbalance
Zoltan_LB_Eval_HG  Number of objects :         3        5       25   1.400
Zoltan_LB_Eval_HG  Object weight     :         3        5       25   1.400

Zoltan_LB_Eval_HG  CUTN (Sum_edges( (#parts(edge)>1)*ewgt )):   24.000
Zoltan_LB_Eval_HG  CUTL (Sum_edges( (#parts(edge)-1)*ewgt )):   37.000
Zoltan_LB_Eval_HG  CUTL-MAX (Max_parts( comm. volume ):         12.000


FILE zdrive.inp.phg.ipm.fixed03:  Total:    1.018131e-01 seconds in Partitioning
FILE zdrive.inp.phg.ipm.fixed03:  Average:  1.018131e-01 seconds per Iteration
